IBML_{MQSeries Three Tier for AIX}

Version 1.0

MQSeries Three Tier for AIX allows you to break client/server applications free from the constraints of departmental LAN-based computing. MQSeries Three Tier for AIX supports three logical layers: presentation logic on the client, business logic on the server, and data logic on an enterprise server. The enterprise server can run any application accessible using MQSeries products, including databases or transaction managers. Application data is transferred between the presentation, business, and data logic layers using MQSeries messages.

MQSeries Three Tier for AIX builds on MQSeries and supports advanced graphical user interfaces (GUIs) allowing extended business interactions. Interactive applications can access many systems using MQSeries, helping the application to continue to give useful and timely responses even when some systems become unavailable.

MQSeries Three Tier for AIX provides an application structure suited to either procedural or object-based design. It allows application designers and programmers to design large, integrated, client/server applications in a way that is straightforward and makes them manageable, extendable, and reusable.

Benefits of MQSeries Three Tier for AIX

• A significant reduction in lines of application code compared to less advanced messaging infrastructures • A technique for the creation of powerful and extensible enterprise client/server applications • Increased chance that application components will be reusable • Improved throughput and

customer service for the enterprise • User-friendly GUI access to LAN-based business logic and new or legacy database applications

Program name

The name of this product is IBM MQSeries Three Tier for AIX Version 1.0

Program number: 5765-321

Hardware requirements

• Any workstation capable of running the required level of AIX and MQSeries for AIX.

• Any communication hardware supported by MQSeries for AIX.

Software requirements

For servers:

• AIX Version 3.2.5 • IBM MQSeries for AIX Version 2 or later, with suitable transmission protocol • IBM DCE Threads for AIX Version 1.1 For OS/2 clients (client code is distributed with the product):

• OS/2 Version 2.1 or Warp • IBM MQSeries for OS/2 Client Support with suitable transmission protocol

For Windows clients (client code is distributed with the product):

• DOS Version 5.0 or above • Microsoft Windows for

Workgroups Version 3.1 or Windows Version 3.1 • IBM MQSeries Windows Client Support with suitable transmission protocol

Supported languages

For server programming:

• IBM CSet + + for AIX 6000

For OS/2 client programming, one or more of:

• IBM VisualAge for Smalltalk V2 for OS/2 • IBM MQSeries Three Tier

VisualAge V3 Support for OS/2 (SupportPac MA3D) • IBM CSet+ + • IBM PL/I Package/2 • IBM MQSeries Three Tier COBOL VisualSet Support for OS/2 (SupportPac MA3C in preparation)

For Windows client programming:

• Microsoft Visual C+ + Professional Edition 1.5

• IBM MQSeries Three Tier Visual BASIC Support for Windows Client (SupportPac MA3B)

For further information

For more information about MQSeries Three Tier for AIX, please contact your local IBM representative.

IBM is the registered trademark of International Business Machines Corporation.

IBM, MQSeries, MQSeries Three Tier, CICS, OS/2, VisualAge, C Set+ + , and AIX are trademarks of International Business Machines Corporation.

Windows is a trademark of Microsoft Corporation.

Produced by: IBM United Kingdom Laboratories MQSeries Development MP 206 Hursley Park Winchester Hampshire SO21 2JN United Kingdom

© International Business Machines Corporation 1995